Thanks everybody for the updates/corrections on this board.

I have so far incorporated the following changes.

Peter Higgins

Added a pull-up resistor connected to the S100 \*RESET signal at K10. Many S100 bus motherboards have the reset line pulled up so in order not to overload the line I have used a 4.7K pullup instead of a 1K.

Also added a 4.7K pullup for Z180\_BUSREQ\* on the SC131 circuit (for John Kennedy).

Roy Bragg, John Kennedy

Changed K6 to a Male DC Power Jack in schematic. I used Jameco #2210677. Can somebody check #297570 also works.

Peter Higgins

Added Silk Screen text for the pinout of the two serial to USB adaptors

Roy Bragg

The resistors are Jameco 1/8 watt resistors Roy. Fairly common/standard. The pinout is from the KiCAD library footprint. I find if I bend them sharp just as the wire comes out of the actual resistor they fit fine.