CLOCK_ENABLE_INPUT_A=BYPASS
CLOCK_ENABLE_OUTPUT_A=BYPASS
INTENDED_DEVICE_FAMILY="Cyclone IV E"
NUMWORDS_A=4096
OPERATION_MODE=SINGLE_PORT
OUTDATA_ACLR_A=NONE
OUTDATA_REG_A=CLOCK1
POWER_UP_UNINITIALIZED=FALSE
READ_DURING_WRITE_MODE_PORT_A=NEW_DATA_NO_NBE_READ
WIDTHAD_A=12
WIDTH_A=8
WIDTH_BYTEENA_A=1
DEVICE_FAMILY="Cyclone IV E"
address_a
clock0
clock1
rden_a
q_a
